=====================================================================
	         Yafuflash Utility Instructions
=====================================================================
We provide several DOS mode batch files for you to update the BMC firmware version, 
as explained below:

1.
FLASH1.BAT : 
run this batch file to flash the BMC firmware and preserve most of the BMC settings.

2.
FLASH2.BAT : 
run this batch file to flash the BMC firmware and force BMC bootloader upgrade. 
Its do not preserve any BMC settings.

3.
ASMB_MAC.exe and ASMC8.exe:
Subprogram for BMC firmware update.

4. 
*.ima : 
Image file of BMC firmware.



If you encounter any problems during the BMC firmware update process, please contact your system
vendor or ASUS Customer Service for support.
