To update firmware of GIGABYTE BMC, we offer tools can be used in a variety of OS: DOS, Windows, Linux.

Files Hierarchy
doc
|--BMCFirmwareUpdate.txt
fw
|--120499.bin               ; Whole 64M Bytes in binary for raw programming or update BMC.
utility
|--fwud
    |--dos
        |--flashAll.bat  ; The batch file was used to update BMC.
        |--socflash.EXE  ; The utility is flash tool for update BMC.
    |--linux
        |--flashall64.sh ; The shell script calls 64bit/bmcfwul to update BMC.
        |--socflash_x64	 ; The utility is flash tool for update BMC.
    |--windows
        |--flashall64.bat  ; The batch file calls 64bit/bmcfwu.exe to update BMC.
        |--socflash_x64.exe; The utility is flash tool for update BMC.
        
Example:
     
        Update BMC - socflash
                cd utility\fwud\dos
                flashAll.bat
                
