Product Name: X10SRL-F
Revision: 2.0b		Previous Revision: 2.0a
Release Date: 4/28/2017
Update Category: Recommended
Dependencies:
None
Important Notes:
None
Enhancements:
1. Updated for Broadwell-EP RC 4.2.0 PLR10 release.
2. Updated Intel Server Platform Services 3.1.3.38 PLR7 for Grantley Refresh Platforms.
3. Updated CPU microcode SRV_P_192 for Broadwell-EP B0/M0/R0.
4. Updated CPU microcode SRV_P_191 for Haswell-EP C0,1/M0,1/R2.
New Features:
1. Added display of Monitor/Mwait setup item in CPU Configuration. 
2. Added ability of MECI (Multiple Event Count Increment) and METW (Multiple Event Time Window) to work with memory correct error and PCIe error reports.
3. Added VB tag to VPD data if not already present.
4. Implemented the IIO bifurcation item.
Fixes:
1. Applied AMI EIP EIP274689 to fix some BIOS setup items not working properly with default values loaded on the CPU page.
2. Fixed issue where changes in METW or MECI values do not take effect in current boot to OS.
3. Corrected MECI help string typo (from "Mutiple" to "Multiple").
4. Fixed system hanging at 0xA9 when the GPNV event log is full.
5. Fixed system hanging at POST 0xB2 when installing Mellanox MCX311a and MCX312C-XCCT.
6. Fixed SUM error when running "GetCurrentBiosCfgTextFile" after BIOS setup modified by AMIBCP.
7. Fixed problem where "Processor Frequency" could not be changed when setting "Boot performance mode" to "Max Efficient" by AMIBCP.
8. Fixed system hanging when plugging in an add-on card that contains non-SMC format VPD data.
9. Fixed multiple event time count not following the specifications.
10. Fixed problem where slot 6 OPROM item doesn’t work.
11. Corrected location of memory error on UP server.
12. Fixed issue with Grantley where Super.rom does not work and SUT hangs on POST 79.