- LAN NVM update package Broadcom BCM57416 10G BASE-T*2.

===================
SEE INSTRUCTION.TXT
===================

EEPROM REVISION INFO:
12) H1xSSx-xT_20240515_229-1-123-0_NUP (5/15/2025)
	a. H11SSW-NT.pkg and H11SSW-NT.pup from SMCCD_v229.1.123.0b_g
		Family version 229.1.123.0
		Firmware version 229.0.141.0
		MBA version 229.0.137.0
	b. This firmware included the fix below:
		ID: DCSG01597124
		Headline: Fixed BMC Temp sensor not working intermittently - This issue is resolved initially in 226.1.107.8 release

11) SSWNT60_NUP (6/21/2023)
	a. H11SSW-NT.pkg and H11SSW-NT.pup from SMCCD_v226.1.107.1a_g
		Family version 226.1.107.1
		Firmware version 226.0.145.0
		MBA version 226.0.135.0
	b. Major issue resolved for this release is when the system gets stuck at root port (CS00012298349).

10) SSWNT5C_NUP (4/14/2023)
	a. H11SSW-NT.pkg and H11SSW-NT.pup - same F/W version as SSWNT5B_NUP
		+ LAN 2 nvm cfg 209 set to 0 to disable it during S5 state.

9) SSWNT5B_NUP (3/15/2023)
	a. H11SSW-NT.pkg and H11SSW-NT.pup from SMCCD_v225.1.95.0a_g
		Family version 225.1.95.0
		Firmware version 225.0.132.0
		MBA version 225.0.144.0

8) SSWNT50_NUP (12/14/2022)
	a. H11SSW-NT.pkg and H11SSW-NT.pup from SMCCD_v224.1.102.0b_g
		Family version 224.1.102.0
		Firmware version 224.0.158.0
		MBA version 224.0.155.0

7) SSWNT4C_NUP (10/14/2022)
	a. H11SSW-NT.pkg and H11SSW-NT.pup from SMCCD_v223.1.96.0_g
		Family version 223.1.96.0
		Firmware version 223.0.161.0

6) SSWNT4B_NUP (2/7/2022)
	a. Based on H11SSW-NT.pkg from SMCCD_v220.0.83.0a_g. 
		Family version 220.0.83.0
		Firmware version 220.0.59.0
	b. H11SSW-NT.pup file for PLDM updating.
	c. Use bnxt_en-1.10.2-220.0.13.0 and bnxtnvm from this NUP package.

5) SSWNT4A_NUP (10/11/2021)
	a. H12SSW-NT.pkg and H12SSW-NT.pup from SMCCD_v218.0.300.0a_g.

4) SSWNT404_NUP (8/19/2021) - Revision 404 to match with production package
	a. H12SSW-NT.pkg with Broadcom VPD.
	b. H12SSW-NT.pup file for PLDM updating.

3) SSWNT401_NUP (4/7/2021)
	a. Modified instruction and requirements. 
	*** NEED TO HAVE LATEST DRIVER bnxt_en-1.10.2-218.0.67.0 AND TOOL bnxtnvm-218.0.54.0 ***

2) SSWNT40_NUP (2/4/2021)
	a. Based on H11SSW-NT.pkg from SMCCD_v218.0.169.0_g. 
		Family version 218.0.169.0
		Firmware version 218.0.153.0 
	b. H11SSW-NT.pup file for PLDM updating.

1) SSWNT3C_NUP (12/14/2020)
	a. Based on H11SSW-NT.pkg (included SMC CFG) from SMCCD_v216.0.416.10_g. 
		Family version 216.0.416.10
		Firmware version 214.4.107.6