================================================================================
Supermicro System BMC Update Package Operation Instructions
================================================================================

Please read this document in it before performing the system BMC update.  
Please verify that your system meets the requirments.

********************************************************************************
This update package includes the following system software updates & utilities:

--- BMC FW image ---

  BMC          - BMC_H12AST2600-ROT-E201MS_20260428_01.06.32_STDsph.bin              (REV 01.06.32)

--- BMC Update Tools ---

  SuperServer Automation Assistant (SAA) UEFI V1.2.0-p1 (2024/10/30) 
 
  SAA.efi                                       (for UEFI)
  README.txt                               (SAA Readme file) 
  UEFI_SAA_UserGuide.pdf        (SAA Readme file) 
  flash.nsh                                     (Update Script)
  command_example.txt            (Example file for using the update script)


--- Supported Products ---

  Supermicro Motherboards:
  MBD-H12DSI-N6/NT6
  

*************************************************************************************
                                     Important notes
*************************************************************************************

1. The UEFI version of SAA tool will replace AMI AFU BMC flash utility in H14 
motherboard BMC.

2. Using AFU tool will end up with the BMC corruption.  It should never be used!


*************************************************************************************
                       SYSTEM HARDWARE and FIRMWARE REQUIREMENTS
*************************************************************************************

<NONE>


*************************************************************************************
                                         Warning
*************************************************************************************

1. Do not interrupt, reboot or remove power from your system during the update.
   Doing so may cause the system failure.

2. If the software update fails, you may contact our RMA Department to have the BIOS/
   IPMI firmware chip reprogrammed.  This will require shipping the board to Supermicro
   for repair.  Please submit your RMA request at:
   http://www.supermicro.com/support/rma/.
