**SMC2008IT firmware Flash Process (PRELIMINARY 9/10/12)**

**Flashing IT mode in DOS:**

1) Please copy all files from DOS folder to bootable USB disk

2) Run SMC2008T.bat and following the instruction to enter the last 9 digits/character of the SAS address.

3) If you are having problem to enter the SAS address, please use the command below to set the controller SAS address.

sas2flsh.exe -o –sasadd “Controller SAS address”

For example: sas2flsh.exe -o –sasadd 50030480070a8b00

4) Reboot the system

**Flashing IT mode in UEFI shell: For all X9 MB**

1) Please copy all files from UEFI folder to bootable USB disk

2) Run SMC2008T.nsh and following the instruction to enter the last 9 digits/character of the SAS address.

3) If you are having problem to enter the SAS address, please use the command below to set the controller SAS address.

sas2flash.efi -o –sasadd “Controller SAS address”

For example: sas2flash.efi -o –sasadd 50030480070a8b00

4) Reboot the system